<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.61" y2="0" width="0" layer="20"/>
<wire x1="54.61" y1="0" x2="54.61" y2="50.8" width="0" layer="20"/>
<wire x1="54.61" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="0" width="0" layer="20"/>
<text>DC Power Out</text>
<text>USB</text>
<text>CANtranslator</text>
<text>R0.3</text>
<text>OpenXC</text>
<text>OBD-II Right-Angle Connector</text>
<hole x="51.562" y="47.752" drill="2.54"/>
<hole x="3.048" y="47.752" drill="2.54"/>
<hole x="51.562" y="3.048" drill="2.54"/>
<hole x="3.048" y="3.048" drill="2.54"/>
<text>BT LED</text>
<text>USB LED</text>
<text>Front Panel LEDS</text>
<text>C13</text>
<text>IC6</text>
<text>ENGR:  Andrew Tergis</text>
<text>Revision 0.3</text>
<text>andrew.tergis@buglabs.net</text>
<text>Bug Labs INC.</text>
<text>www.buglabs.net</text>
<text>1.  All dimensions are in Inches unless otherwise specified</text>
<text>2.  Finished board thickness 0.061 inches +/- 0.006" </text>
<text>3.  PCB Construction:  Std. 2-layer stackup, 0.5oz CU</text>
<text>4.  Soldermask over bare copper, both sides</text>
<text>5.  Silkscreen on TOP side only, clip from solder lands</text>
<text>6.  Minimum Conductor Width/Spacing:  8mil</text>
<text>7.  PCB Material: FR-4 or equivalent</text>
<text>8.  Files are in Gerber 274X format</text>
<text>9.  Finished PCB Warpage and Twist per IPC-6012</text>
<text>10. Layer to layer registration variation +/- 0.005"</text>
<text>11. Hole size variation +/- 0.004" of the finished drill size</text>
<text>12. Board outline variation +/- 0.010" of board outline layer</text>
<text>13. Remove all burrs if present</text>
<text>NOTES:</text>
<text>SJ3</text>
<text>SJ4</text>
<text>LED1</text>
<text>LED4</text>
<text>C3</text>
<text>C2</text>
<text>J4</text>
<text>J1</text>
<text>J2</text>
<text>J5</text>
<text>14. All through hole components installed on bottom side</text>
<text>C9</text>
<text>C22</text>
<text>FB1</text>
<text>SJ6</text>
<text>C10</text>
<text>D7</text>
<text>D6</text>
<text>D2</text>
<text>J3</text>
<text>R25B</text>
<text>TP4</text>
<text>TP7</text>
<text>TP8</text>
<text>TP9</text>
<text>TP10</text>
<text>TP11</text>
<text>TP13</text>
<text>TP6</text>
<text>TP12</text>
<text>TP21</text>
<text>TP19</text>
<text>TP20</text>
<text>TP3</text>
<text>TP2</text>
<text>TP1</text>
<text>TP5</text>
<text>TP22</text>
<text>TP14</text>
<text>TP23</text>
<text>TP15</text>
<text>TP16</text>
<text>TP17\</text>
<text>TP18</text>
<text>15. Solder on shield of J1 (USB Micro) must not be</text>
<text>wicked into the path of the connector</text>
<text>17. LED1+LED4 must be bent 90 degrees towards edge of PCB, overhang ok</text>
<text>18. Electrolytic caps to be soldered flush on PCB - no exposed leads</text>
<text>D8</text>
<text>D9</text>
<text>D10</text>
<text>F1</text>
<text>16. Ensure J1 (USB Micro) is soldered flush to the PCB</text>
<text>LAYER-STACK</text>
<text>01-16</text>
<text>01-20</text>
<text>J3</text>
<text>GND</text>
<text>GND</text>
<text>JP2</text>
</plain>
<libraries>
<library name="BUG">
<packages>
<package name="TQFP100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package Outline&lt;/b&gt;</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED-0603">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SMB-DIODE">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
Basic small signal diode good up to 200mA. SMB footprint. Common part #: BAS16</description>
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="ST2012SB">
</package>
<package name="CX3225SB">
</package>
<package name="SO14">
</package>
<package name="SHF-105-01-X-D-SM">
<description>0.050"X0.050" SHROUDED TERMINAL STRIP ASSEMBLY, 10PINS.</description>
</package>
<package name="CPOL-10MMX5D">
</package>
<package name="CPOL-5MMX2D">
</package>
<package name="POWER_SO8">
</package>
<package name="2-1445055-2">
</package>
<package name="OBDII-COMTECH">
</package>
<package name="LED5MM-RGB">
</package>
<package name="10118193">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1210">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOD-882">
</package>
<package name="SOD-882D">
</package>
<package name="SOT-1123">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="PAD.03X.05">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RN41">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="V-REG_DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="frames">
<description>&lt;b&gt;Frames for Sheet and Layout&lt;/b&gt;</description>
<packages>
<package name="A4L-LOC">
<description>&lt;b&gt;FRAME&lt;/b&gt; DIN A4 landscape with doc field</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="drilegend">
<packages>
<package name="DRILEGEND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC5" library="BUG" package="TQFP100" value="LPC1769FBD100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C19" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C18" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C17" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C16" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C15" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="C14" library="BUG" package="0805" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="IC6" library="SparkFun-RF" package="RN41" value="RN41-I/RM"/>
<element name="C21" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="LED3" library="BUG" package="LED-0603" value="SML-LX0603SRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="BUG" package="0402-RES" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="BUG" package="0402-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="BUG" package="0402-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="BUG" package="SOT23" value="PESD1CAN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="BUG" package="SOT23" value="PESD1CAN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SparkFun-PowerIC" package="V-REG_DPACK" value="TLE4284DV33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="BUG" package="0805" value="0.47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="BUG" package="0805" value="0.47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="BUG" package="SMB-DIODE" value="1SMB16CAT3G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="BUG" package="0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="BUG" package="0805" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C11" library="BUG" package="0402-CAP" value="22n">
<attribute name="NAME"/>
</element>
<element name="IC1" library="SparkFun-PowerIC" package="V-REG_DPACK" value="LM340S-50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="BUG" package="SMA-DIODE" value="RS1J">
<attribute name="NAME"/>
</element>
<element name="C1" library="BUG" package="0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="BUG" package="0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="BUG" package="0402-CAP" value="22n">
<attribute name="NAME"/>
</element>
<element name="R16" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="Q2" library="BUG" package="ST2012SB" value="32k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="BUG" package="0402-CAP" value="18p">
<attribute name="NAME"/>
</element>
<element name="C25" library="BUG" package="0402-CAP" value="18p">
<attribute name="NAME"/>
</element>
<element name="Q3" library="BUG" package="CX3225SB" value="12M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="BUG" package="0402-CAP" value="18p">
<attribute name="NAME"/>
</element>
<element name="C26" library="BUG" package="0402-CAP" value="18p">
<attribute name="NAME"/>
</element>
<element name="IC3" library="BUG" package="SO14" value="TJA1048T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="BUG" package="0402-RES" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="BUG" package="SHF-105-01-X-D-SM" value="ARM mini-JTAG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="BUG" package="0402-RES" value="33E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="BUG" package="0402-RES" value="33E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="BC856">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="BUG" package="0402-RES" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="BUG" package="0402-RES" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="BUG" package="LED-0603" value="SML-LX0603SRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="BUG" package="0402-RES" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="BUG" package="CPOL-10MMX5D" value="270u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="BUG" package="CPOL-5MMX2D" value="150u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-TRACE" value="CLOSED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="SJ_2S-TRACE" value="CLOSED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="BUG" package="POWER_SO8" value="TPS2421-2">
<attribute name="NAME"/>
</element>
<element name="R18" library="BUG" package="0402-RES" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="BUG" package="0402-CAP" value="1u">
<attribute name="NAME"/>
</element>
<element name="J4" library="BUG" package="2-1445055-2" value="PWR OUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="BUG" package="0402-RES" value="17.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="BUG" package="0402-RES" value="30">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="BUG" package="0402-RES" value="143">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="BUG" package="OBDII-COMTECH" value="OBDII"/>
<element name="R20" library="BUG" package="0402-RES" value="143">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="BUG" package="0402-RES" value="30">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="BUG" package="0402-RES" value="17.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun-Passives" package="SJ_3_PASTE1&amp;2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="SparkFun-Passives" package="SJ_3_PASTE1&amp;2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="BUG" package="LED5MM-RGB" value="RGB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="BUG" package="LED5MM-RGB" value="RGB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="PROG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="BUG" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="ISP_EN">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="ISP">
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="SparkFun-Passives" package="SJ_2S-NO" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="BUG" package="0402-CAP" value="100p">
<attribute name="NAME"/>
</element>
<element name="C30" library="BUG" package="0402-CAP" value="100p">
<attribute name="NAME"/>
</element>
<element name="C31" library="BUG" package="0402-CAP" value="100p">
<attribute name="NAME"/>
</element>
<element name="C32" library="BUG" package="0402-CAP" value="100p">
<attribute name="NAME"/>
</element>
<element name="C33" library="BUG" package="0402-CAP" value="100p">
<attribute name="NAME"/>
</element>
<element name="C34" library="BUG" package="0402-CAP" value="100p">
<attribute name="NAME"/>
</element>
<element name="R25" library="BUG" package="0402-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="BUG" package="10118193" value="USB_MINIB_SHIELD-10118193">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ZDRAW1" library="frames" package="A4L-LOC" value=""/>
<element name="R25B" library="BUG" package="AXIAL-0.4" value="DNP"/>
<element name="TP1" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP2" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP3" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP4" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP5" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP6" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP7" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP8" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP9" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP10" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP11" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP12" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP13" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP14" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP15" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP16" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP17" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP18" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP19" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP20" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP21" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="C9" library="BUG" package="1210" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP22" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP23" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="C10" library="BUG" package="0402-CAP" value="0.1u">
<attribute name="NAME"/>
</element>
<element name="SJ6" library="SparkFun-Passives" package="SJ_2S-TRACE" value="CLOSED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="BUG" package="C0402" value="742843122">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="BUG" package="0402-CAP" value="1u">
<attribute name="NAME"/>
</element>
<element name="D7" library="BUG" package="SOD-882" value="PESD5V0X1BL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="BUG" package="SOD-882" value="PESD5V0X1BL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="BUG" package="SOD-882D" value="PESD12VS1ULD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="F1" library="adafruit" package="R1206" value="MF-MSMF110/16-2"/>
<element name="D8" library="BUG" package="SOT-1123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="BUG" package="SOT-1123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="BUG" package="SOT-1123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DRILEGEND" library="drilegend" package="DRILEGEND" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC5" pad="83"/>
<contactref element="IC5" pad="31"/>
<contactref element="IC5" pad="55"/>
<contactref element="IC5" pad="72"/>
<contactref element="IC5" pad="97"/>
<contactref element="IC5" pad="41"/>
<contactref element="IC5" pad="15"/>
<contactref element="IC5" pad="11"/>
<contactref element="C21" pad="1"/>
<contactref element="IC6" pad="29"/>
<contactref element="IC6" pad="28"/>
<contactref element="IC6" pad="27"/>
<contactref element="IC6" pad="25"/>
<contactref element="IC6" pad="12"/>
<contactref element="IC6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="D5" pad="3"/>
<contactref element="C12" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="D4" pad="3"/>
<contactref element="R17" pad="2"/>
<contactref element="J5" pad="9"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="5"/>
<contactref element="R18" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC7" pad="PAD"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="5"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED4" pad="2"/>
<contactref element="S2" pad="P$1"/>
<contactref element="JP2" pad="2"/>
<contactref element="J3" pad="6"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="S1" pad="P$1"/>
<contactref element="R25" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="S1"/>
<contactref element="J1" pad="S2"/>
<contactref element="C13" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="R25B" pad="P$1"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C22" pad="1"/>
<contactref element="D7" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="D8" pad="3"/>
<contactref element="D9" pad="3"/>
<contactref element="D10" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="IC2" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="IC3" pad="11"/>
<contactref element="R15" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="IC5" pad="28"/>
<contactref element="IC5" pad="54"/>
<contactref element="IC5" pad="71"/>
<contactref element="IC5" pad="96"/>
<contactref element="IC5" pad="84"/>
<contactref element="IC5" pad="42"/>
<contactref element="IC5" pad="12"/>
<contactref element="IC5" pad="10"/>
<contactref element="R24" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="J3" pad="4"/>
<contactref element="R19" pad="1"/>
<contactref element="TP7" pad="P$1"/>
<contactref element="C9" pad="1"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="TP6" pad="P$1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="CANA_TX">
<contactref element="IC5" pad="56"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="CANA_RX">
<contactref element="IC5" pad="57"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="CANB_RX">
<contactref element="IC5" pad="81"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="CANB_TX">
<contactref element="IC5" pad="80"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="+12V">
<contactref element="C7" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="D1" pad="A"/>
<contactref element="IC7" pad="3"/>
<contactref element="J2" pad="16"/>
<contactref element="TP5" pad="P$1"/>
</signal>
<signal name="BT_CONN">
<contactref element="IC6" pad="19"/>
<contactref element="IC5" pad="60"/>
<contactref element="TP13" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="IC6" pad="21"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="BT_RX">
<contactref element="IC6" pad="13"/>
<contactref element="IC5" pad="62"/>
<contactref element="TP8" pad="P$1"/>
</signal>
<signal name="BT_TX">
<contactref element="IC6" pad="14"/>
<contactref element="IC5" pad="63"/>
<contactref element="TP9" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="C12" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="C13" pad="1"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="C5" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC5" pad="18"/>
<contactref element="Q2" pad="1"/>
<contactref element="C25" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="IC5" pad="16"/>
<contactref element="Q2" pad="2"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="IC5" pad="22"/>
<contactref element="Q3" pad="3"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="IC5" pad="23"/>
<contactref element="Q3" pad="1"/>
<contactref element="C28" pad="1"/>
</signal>
<signal name="TRST">
<contactref element="IC5" pad="4"/>
<contactref element="R15" pad="2"/>
<contactref element="D8" pad="1"/>
</signal>
<signal name="TDI">
<contactref element="IC5" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="J5" pad="8"/>
<contactref element="D9" pad="1"/>
</signal>
<signal name="TMS">
<contactref element="IC5" pad="3"/>
<contactref element="R13" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="D8" pad="2"/>
</signal>
<signal name="TCK">
<contactref element="IC5" pad="5"/>
<contactref element="R17" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="D10" pad="1"/>
</signal>
<signal name="RTCK">
<contactref element="IC5" pad="100"/>
<contactref element="R12" pad="2"/>
<contactref element="J5" pad="7"/>
<contactref element="D10" pad="2"/>
</signal>
<signal name="TDO">
<contactref element="IC5" pad="1"/>
<contactref element="J5" pad="6"/>
<contactref element="D9" pad="2"/>
</signal>
<signal name="DEBUG_TX">
<contactref element="IC5" pad="98"/>
<contactref element="J3" pad="2"/>
<contactref element="TP19" pad="P$1"/>
</signal>
<signal name="DEBUG_RX">
<contactref element="IC5" pad="99"/>
<contactref element="J3" pad="3"/>
<contactref element="TP20" pad="P$1"/>
</signal>
<signal name="USB_D+">
<contactref element="IC5" pad="29"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="USB_D-">
<contactref element="IC5" pad="30"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R10" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="D7" pad="2"/>
</signal>
<signal name="USB_VBUS">
<contactref element="IC5" pad="21"/>
<contactref element="J1" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="R8" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$28">
<contactref element="R11" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$29">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="USB_CON">
<contactref element="R9" pad="2"/>
<contactref element="IC5" pad="64"/>
<contactref element="TP16" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SJ2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC7" pad="5"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC7" pad="6"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="IC7" pad="7"/>
<contactref element="TP15" pad="P$1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="2"/>
<contactref element="LED4" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="R6" pad="2"/>
<contactref element="LED4" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="R5" pad="2"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC5" pad="40"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC5" pad="38"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC5" pad="37"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R22" pad="2"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="R21" pad="2"/>
<contactref element="LED1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R20" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC7" pad="2"/>
<contactref element="IC5" pad="50"/>
<contactref element="TP14" pad="P$1"/>
</signal>
<signal name="BT_RTS">
<contactref element="IC6" pad="15"/>
<contactref element="IC5" pad="73"/>
<contactref element="TP10" pad="P$1"/>
</signal>
<signal name="BT_CTS">
<contactref element="IC6" pad="16"/>
<contactref element="IC5" pad="66"/>
<contactref element="TP11" pad="P$1"/>
</signal>
<signal name="MULTI_HI">
<contactref element="J2" pad="1"/>
<contactref element="SJ3" pad="3"/>
<contactref element="C29" pad="1"/>
</signal>
<signal name="MSPD_HI">
<contactref element="J2" pad="3"/>
<contactref element="SJ3" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="D5" pad="2"/>
<contactref element="IC3" pad="10"/>
<contactref element="R2" pad="2"/>
<contactref element="SJ3" pad="2"/>
<contactref element="TP3" pad="P$1"/>
</signal>
<signal name="MULTI_LO">
<contactref element="J2" pad="8"/>
<contactref element="SJ4" pad="3"/>
<contactref element="C33" pad="1"/>
</signal>
<signal name="MSPD_LO">
<contactref element="J2" pad="11"/>
<contactref element="SJ4" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="IC3" pad="9"/>
<contactref element="SJ2" pad="2"/>
<contactref element="SJ4" pad="2"/>
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="HSPD_HI">
<contactref element="J2" pad="6"/>
<contactref element="IC3" pad="13"/>
<contactref element="D4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="HSPD_LO">
<contactref element="J2" pad="14"/>
<contactref element="IC3" pad="12"/>
<contactref element="D4" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="IC5" pad="32"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="IC5" pad="34"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="IC5" pad="35"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="!ISP_EN">
<contactref element="IC5" pad="53"/>
<contactref element="R23" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="TP17" pad="P$1"/>
</signal>
<signal name="!USBBOOT_EN">
<contactref element="IC5" pad="51"/>
<contactref element="R24" pad="2"/>
<contactref element="S2" pad="P$2"/>
<contactref element="TP18" pad="P$1"/>
</signal>
<signal name="N$36">
<contactref element="J3" pad="1"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R19" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="R25" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="R25B" pad="P$2"/>
</signal>
<signal name="!RESET">
<contactref element="IC5" pad="17"/>
<contactref element="C23" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="S1" pad="P$2"/>
<contactref element="TP21" pad="P$1"/>
<contactref element="J5" pad="10"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="CANA_EN">
<contactref element="IC3" pad="14"/>
<contactref element="IC5" pad="59"/>
</signal>
<signal name="CANB_EN">
<contactref element="IC3" pad="8"/>
<contactref element="IC5" pad="79"/>
</signal>
<signal name="!BT_RST">
<contactref element="TP12" pad="P$1"/>
<contactref element="IC5" pad="61"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="IC7" pad="1"/>
<contactref element="TP22" pad="P$1"/>
</signal>
<signal name="N$35">
<contactref element="TP23" pad="P$1"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="N$37">
<contactref element="SJ6" pad="2"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$38">
<contactref element="FB1" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="IC6" pad="11"/>
<contactref element="C22" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
